{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":6,"rows_kept":16,"merged":[[0,0,3,5],[9,2,15,5]]}
["车间出入口现场监控屏系统采购需求明细表"]
[]
[]
[]
["品名","规格","单位","数量","单价","金额（元）"]
["55寸电视机","屏幕分辨率不低于4K；尺寸≥55英寸，≤60英寸；比例16:9；存储内存≥32GB；CPU不低于四核；系统基于Android；运行内存≥2GB；HDMI2.0接口≥2个。","台",31]
["媒体交换\n服务器","处理器性能满足多路音视频流处理需求；支持主流Linux操作系统；内存≥8GB；硬盘支持≥4盘位，系统盘≥8T；网口≥千兆口×3；支持PCI-E扩展；具备音视频流复制、分发、转发能力，支持负载均衡与冗余备份；★需接入我司现有监控平台，支持远程配置与管理。","台",1]
["解码器","支持7×24小时稳定运行；支持同时解码不少于4路4K@30帧、16路1080P@30帧；支持H.265/H.264等格式；支持1路视频输出，输出分辨率最高支持4K@60Hz；★接入我司现有监控系统。","台",8]
["解码器","支持7×24小时稳定运行；具备不少于2路HDMI输入；支持解码不少于20路1080P@30帧；支持H.265/H.264等格式；支持1-16分屏显示与画面拼接；支持4路视频输出，输出分辨率最高支持4K@60Hz；★接入我司现有监控系统。","台",4]
["信号延长器","支持单网线130米传输HDMI2.0信号，4K*2K@60Hz，\n支持HDR，支持HDCP,铝合金盒HDMI网络延长器 \nHDMI信号：HDMI1.4且兼容HDCP1.4协议 \n音视频同步传输   1080P 1收1发 \n分辨率：1080P，且向下兼容视频放大宽带1.65Gbps/165Hz \n视频放大宽带：1.65Gbps/165Hz 功 耗： 3W HDMI信号：HDMI1.4且兼容HDCP1.4协议 ","本部分包干，包安装调试到位。"]
["支架","1米吊装支架 360度旋转自由伸缩，加固不掉落 \n适用电视安装32-75英寸电视机隐藏式束线孔 "]
["管材","规格：16mm≤外径≤25mm "]
["电源线","RVV 2*1.0 ，无氧铜 200米/卷"]
["网络线","六类网线  300米无氧铜4*2*0.55"]
["辅材","根据现场需求提供产品辅材"]
["安装调试","包含设备安装、系统调试、布线、测试及基础培训等服务。"]